睇下portc 邊個bit 係0

Loop

用wait\_press, wait\_up睇有冇用到

用咗去聲

Cblock store freq of tone